

**Detail Specifications：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model No.** | **DGO9748CD** | | |
| Sensivity(0dB=1v/μbar,1KHz) | -36dB ～ -46dB | Operation   Voltage(Max./Std.) | 4.5V |
| Impedance | Low impedance(2.2KΩ-30% ) | Resistance(RL): | 2.2KΩ |
| Directivity | Omni-directinal | Current Consumption: | Max.0.5.mA |
| Frequency | 20~16，000Hz | Sensitivity Reduction | Within -3dB at 1.5V |
| Max.operation voltage | 10V | S/N Ratio | More than 58dB |