|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **Parameters：**  http://www.china-epe.com/admin/editor/attached/image/20120730/20120730131777117711.jpg  **Detail Specifications:**   |  |  |  |  | | --- | --- | --- | --- | | **Model No.** | **DGO6050CD** | | | | Sensivity(0dB=1v/μbar,1KHz) | -36dB ～ -46dB | Operation   Voltage(Max./Std.) | 4.5V | | Impedance | Low impedance(2.2KΩ-30% ) | Resistance(RL): | 2.2KΩ | | Directivity | Omni-directinal | Current Consumption: | Max.0.5.mA | | Frequency | 20~16，000Hz | Sensitivity Reduction | Within -3dB at 3V | | Max.operation voltage | 10V | S/N Ratio | More than 60dB | | |